**Product Fiche**

**Supplier Name / Trademark** THE COLLECTION

**Suppliers Model Identifier** DPRLGISN3 CELENA SC MK3 NG

**Energy Efficiency Class** E

**Direct Heat Output (Net)** 4.0 kW

**Indirect Heat Output** Not applicable

**Energy Efficiency Index** 67 %

**Useful Energy Efficiency** 76.3 %

This appliance must be installed in accordance with the rules in force and used in a well-ventilated space. Consult the instructions before installation and use of the appliance.